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At a glance.
· [image: ]Success model BMW X1: more than 275 000 units sold worldwide to date; more milestones through US market launch and start of production in China; comprehensive further development of the first BMW X model for the premium compact segment; new BMW X1 embarks on a continuation of its success story with specially modified body styling, a significantly enhanced interior, state-of-the-art drive technology and innovative equipment features.
· Targeted design accents to reinforce the vehicle’s character as defined by spontaneous agility, urban elegance and robust versatility in the mould of BMW X models; front apron with new structure and extended painted surfaces emphasises affiliation to the family of BMW X models and premium feel; new headlight design with LED accent lights and LED light rings for the LED daytime running lights in conjunction with optional Xenon lights; new foglamp surrounds; reduced plastic bordering at the lower edge of the body; side indicators integrated into the exterior mirrors; larger painted surfaces and more prominent underguard at the rear; new exterior paint colours and alloy wheels.
· Optimised premium feel in the interior thanks to newly designed centre console more clearly orientated towards the driver, refined surfaces and controls, as well as new, particularly high-grade interior trim; optional
new-design sports leather steering wheel.
· BMW Lines available on a BMW X model for the first time; targeted individualisation through exclusive, harmoniously matched design and equipment features; BMW xLine accentuates the robust diversity of the new BMW X1, BMW Sport Line emphasises its agility and dynamics;
BMW Lines as an alternative to the basic trim level; M Sport package available as a further option.


· Engine portfolio expanded by additional units featuring
BMW TwinPower Turbo technology; output range from 85 kW in the BMW X1 sDrive16d to 180 kW in the BMW X1 xDrive28i;
BMW X1 xDrive25d with 160 kW now tops the engine line-up among the diesel models; enhanced performance on the BMW X1 sDrive20d and BMW X1 xDrive20d; new manual transmission with dry sump lubrication; eight-speed automatic transmission unique in this vehicle segment, including Auto Start-Stop function as an option for all models except the BMW X1 sDrive18i (optional six-speed automatic), the BMW X1 sDrive16d and the BMW X1 sDrive20d EfficientDynamics Edition.
· Comprehensive integration of BMW EfficientDynamics technology:
Auto Start-Stop function for manual models as well as those with eight-speed automatic transmission, ECO PRO mode (optional), Brake Energy Regeneration, Electric Power Steering, Optimum Shift Indicator, disengageable climate compressor; BMW X1 sDrive20d EfficientDynamics Edition is the world’s most economical premium vehicle of its kind boasting further honed balance between performance and fuel consumption; further engine variants with significantly reduced fuel consumption (up to 0.9 litres per 100 kilometres on diesel models with eight-speed automatic transmission).
· Intelligent BMW xDrive all-wheel drive standard for two engine variants and optional – and as an alternative to brand-typical rear-wheel drive –
for four variants; electronically controlled, variable power distribution for optimised traction, directional stability and dynamics when cornering;
new efficiency and weight-optimised power divider.
· High-grade suspension technology with double-joint thrust bar or double-joint spring strut axle at the front and five-arm rear axle; speed-sensitive power steering as an option; DSC (Dynamic Stability Control) featuring DTC (Dynamic Traction Control) as standard and Performance Control
as an option.
· Exceptionally solid body structure, comprehensive safety equipment including six airbags and three-point inertia-reel belts on all seats.
· Spacious interior allowing versatile use; three generously sized seats in the rear; 40 : 20 : 40 split-folding rear seatback sections can be individually adjusted in ten stages from 1° to 31°; luggage space with seatback in normal position 420 litres, in comfort position (31°) 360 litres, in cargo position (1°) 480 litres; extendable up to 1 350 litres with the rear seatback fully folded down; wide variety of stowage compartments, trays and cup holders in the passenger compartment.
· Comprehensive standard equipment including climate control, electrically adjustable heated exterior mirrors, foglamps, onboard computer, plus sound system with CD player, AUX-IN connection and five speakers;
high-grade optional equipment, including Professional navigation system with hard disk and iDrive operating system, Harman Kardon Surround Sound System, Comfort Access, Automatic Climate Control, panorama glass roof, automatically dimming exterior and rear-view mirrors, electrically operated seat adjustment, rain sensor, heated steering wheel, tow bar.
· Wide range of optional driver assistance systems and mobility services from BMW ConnectedDrive: High-Beam Assistant, Adaptive Headlights, rear-view camera, Cruise Control with braking function, Internet use, extended smartphone and music player integration, Real Time Traffic Information, as well as BMW apps for receiving web radio and use of Facebook and Twitter.
· 	Model variants:
BMW X1 xDrive28i: BMW TwinPower Turbo technology, comprising twin-scroll turbocharger, High Precision Direct Injection, VALVETRONIC variable valve timing and double VANOS, 
Displacement: 1 997 cc, output: 180 kW at 5 000 – 6 500 rpm, 
max. torque: 350 Nm at 1 250 – 4 800 rpm, 
Acceleration [0 – 100 km/h]: 6.1 (automatic: 6.5) seconds,
top speed: 240 km/h, 
Average fuel consumption: 7.7 – 7.8 litres (7.2 – 7.3 litres)/100 km,
CO2 emissions: 179 – 182 g/km (168 – 171 g/km), exhaust standard: EU5.	

BMW X1 xDrive20i: four-cylinder in-line petrol engine with
BMW TwinPower Turbo technology, comprising twin-scroll turbocharger, High Precision Direct Injection, VALVETRONIC variable valve timing and double VANOS,
Displacement: 1 997 cc, output: 135 kW at 5 000 – 6 250 rpm, 
max. torque: 270 Nm at 1 250 – 4 500 rpm, 
Acceleration [0 – 100 km/h]: 7.8  (automatic: 7.9) seconds,
top speed: 215 km/h, 
Average fuel consumption: 7.5 – 7.7 (7.1 – 7.3) litres/100 km,
CO2 emissions: 176 g/km (167 g/km), exhaust standard: EU5.

BMW X1 sDrive20i: four-cylinder in-line petrol engine with
BMW TwinPower Turbo technology, comprising twin-scroll turbocharger, High Precision Direct Injection, VALVETRONIC variable valve timing and double VANOS, 
Displacement: 1 997 cc, output: 135 kW at 5 000 – 6 250 rpm, 
max. torque: 270 Nm at 1 250 – 4 500 rpm, 
Acceleration [0 – 100 km/h]: 7.4 (automatic: 7.7) seconds,
top speed: 220 km/h, 
Average fuel consumption: 6.9 – 7.1 (6.7 – 6.8 ) litres)/100 km,
CO2 emissions: 162 g/km (157 g/km), exhaust standard: EU5.

BMW X1 sDrive18i: four-cylinder in-line petrol engine with VALVETRONIC variable valve timing and double VANOS, 
Displacement: 1 995 cc, output: 110 kW at 6 400 rpm, 
max. torque: 200 Nm at 3 600 rpm, 
Acceleration [0 – 100 km/h]: 9.7 (automatic: 10.4) seconds,
top speed: 202 km/h / 125 mph (200 km/h), 
Average fuel consumption: 7.7 (7.9) litres/100 km,
CO2 emissions: 180 g/km (185 g/km), exhaust standard: EU5.

BMW X1 xDrive25d: four-cylinder in-line diesel engine with
BMW TwinPower Turbo technology, comprising two turbochargers (Variable Twin Turbo) and common-rail direct injection with piezo injectors (max. injection pressure: 2 000 bar),
Displacement: 1 995 cc, output: 160 kW at 4 000 rpm, 
max. torque: 450 Nm at 1 500 – 2 500 rpm, 
Acceleration [0 – 100 km/h]: 6.8 seconds,
top speed: 230 km/h (automatic: 228 km/h), 
Average fuel consumption: 5.9 (5.5) litres/100 km (47.9 [51.4] mpg imp),
CO2 emissions: 154 g/km (145 g/km), exhaust standard: EU5. 

BMW X1 xDrive20d: four-cylinder in-line diesel engine with
BMW TwinPower Turbo technology package, comprising turbocharger with variable intake geometry, common-rail direct injection with solenoid injectors (max. injection pressure: 1 800 bar),
Displacement: 1 995 cc, output: 135 kW at 4 000 rpm, 
max. torque: 380 Nm at 1 750 – 2 750 rpm, 
Acceleration [0 – 100 km/h]: 8.1 seconds,
top speed: 215 km/h / 133 mph (automatic: 213 km/h), 
Average fuel consumption: 5.5 (5.4) litres/100 km,
CO2 emissions: 145 g/km (143 g/km), exhaust standard: EU5. 

	BMW X1 sDrive20d: four-cylinder in-line diesel engine with
BMW TwinPower Turbo technology package, comprising turbocharger with variable intake geometry, common-rail direct injection with solenoid injectors (max. injection pressure: 1 800 bar),
Displacement: 1 995 cc, output: 135 kW at 4 000 rpm, 
max. torque: 380 Nm at 1 750 – 2 750 rpm, 
Acceleration [0 – 100 km/h / 62 mph]: 7.8 (automatic: 7.9) seconds,
top speed: 220 km/h /136 mph (218 km/h), 
Average fuel consumption: 4.9 (5.0) litres/100 km,
CO2 emissions: 129 g/km (132 g/km), exhaust standard: EU5. 

BMW X1 sDrive20d EfficientDynamics Edition: four-cylinder in-line diesel engine with BMW TwinPower Turbo technology package, comprising turbocharger with variable intake geometry, common-rail direct injection with solenoid injectors (max. injection pressure: 1 800 bar),
Displacement: 1 995 cc, output: 120 kW at 4 000 rpm, 
max. torque: 380 Nm at 1 750 – 2 750 rpm, 
Acceleration [0 – 100 km/h]: 8.3 seconds,
top speed: 215 km/h, 
Average fuel consumption: 4.5 litres/100 km,
CO2 emissions: 119 g/km, exhaust standard: EU5.

	BMW X1 xDrive18d: four-cylinder in-line diesel engine with
BMW TwinPower Turbo technology package, comprising turbocharger with variable intake geometry, common-rail direct injection with solenoid injectors (max. injection pressure: 1 600 bar),
Displacement: 1 995 cc, output: 105 kW at 4 000 rpm, 
max. torque: 320 Nm at 1 750 – 2 750 rpm, 
Acceleration [0 – 100 km/h]: 9.9 (automatic: 10.1) seconds,
top speed: 195 km/h, 
Average fuel consumption: 5.5 (5.4) litres/100 km,
CO2 emissions: 144 g/km (143 g/km), exhaust standard: EU5. 

BMW X1 sDrive18d: four-cylinder in-line diesel engine with
BMW TwinPower Turbo technology package, comprising turbocharger with variable intake geometry, common-rail direct injection with solenoid injectors (max. injection pressure: 1 600 bar),
Displacement: 1 995 cc, output: 105 kW at 4 000 rpm, 
max. torque: 320 Nm at 1 750 – 2 750 rpm, 
Acceleration [0 – 100 km/h]: 9.6 (automatic: 9.9) seconds,
top speed: 202 km/h, 
Average fuel consumption: 4.9 (5.0) litres/100 km,
CO2 emissions: 128 g/km (132 g/km), exhaust standard: EU5. 

BMW X1 sDrive16d: four-cylinder in-line diesel engine with
BMW TwinPower Turbo technology package, comprising turbocharger with variable intake geometry, common-rail direct injection with solenoid injectors (max. injection pressure: 1 600 bar),
Displacement: 1 995 cc, output: 85 kW at 4 000 rpm, 
max. torque: 260 Nm at 1 750 – 3 000 rpm, 
Acceleration [0 – 100 km/h]: 11.5 seconds,
top speed: 190 km/h, 
Average fuel consumption: 4.9 litres/100 km,
CO2 emissions: 128 g/km, exhaust standard: EU5. 

* Figures based on EU test cycle, dependent on tyre format selected.
Geared up for new challenges:
The new BMW X1.
[image: ]As the first premium vehicle of its kind, the BMW X1 is a true trailblazer in the compact segment. After some two-and-a-half years, sales of the compact BMW X model built at BMW Plant in Leipzig and in Tiexi, China have already exceeded 275 000 units. Now this all-round talent emerges with renewed vigour to meet a raft of new challenges. With its specially modified body design, meticulously upgraded interior, comprehensively revised engine portfolio, the new range of BMW Lines and further innovative equipment features, the new BMW X1 delivers an even more intensive experience of the hallmark driving pleasure for which the brand is known.
In parallel with the launch of the new BMW X1, preparations are under way for its US market launch. Further growth impulses emanate from production in China: the new BMW X1 models destined for the Chinese market are being built in the newly opened plant at Tiexi in Shenyang Province.
The successful concept of transferring familiar BMW X features to the compact segment has since led to increased competition in the vehicle class spawned by the BMW X1. What remains uncontested is the BMW X1’s leadership position in terms of sportiness and efficiency. This lead is now being extended: the relationship between performance and fuel consumption has been further optimised thanks to engines with BMW TwinPower Turbo technology, an eight-speed automatic transmission that is unique in this segment, the Auto Start-Stop function, Brake Energy Regeneration,
ECO PRO mode and a wider range of BMW EfficientDynamics technology. Setting a particularly impressive example here is the BMW X1 sDrive20d EfficientDynamics Edition with average fuel consumption in the EU test cycle of 4.5 litres per 100 kilometres and CO2 figures of 119 grams per kilometre.
The range of engines for the new BMW X1 comprises three petrol and five diesel units spanning an output range of 85 kW to 180 kW. Leading the way in the new generation of four-cylinder diesel engines is the 160 kW powerplant of the new BMW X1 xDrive25d, featuring
BMW TwinPower Turbo technology comprising latest-generation variable sequential turbocharging. Depending on the model variant, power is transferred via brand-typical rear-wheel drive or via the intelligent
BMW xDrive all-wheel-drive system. Either option is available to three
of the engine variants of the new BMW X1.
The new BMW X1 also offers innovative individualisation possibilities for the exterior and the interior. Available for the first time, as an alternative to the basic trim level, are the BMW Lines with their exclusive, harmoniously matched design and equipment features. The BMW xLine particularly emphasises the robust versatility of the new BMW X1 while the
BMW Sport Line accentuates its agility and dynamics.
Design: new touches highlight its elegance, versatility and sportiness.
Typical BMW proportions, expressive, vibrant surfaces and signature
BMW X model design cues shape the appearance of the BMW X1.
A sweeping bonnet, long wheelbase and set-back passenger compartment emphasise the car’s dynamic talent, while attractive light and shade effects hint at its inherent agility. The versatility and sturdiness of a BMW X model are reflected in elements such as the black bordering at the lower edge of the body and the muscular wheel arches.
Above all, the new BMW X1 conveys even more strikingly the powerful stance that also distinguishes BMW’s Sports Activity Vehicles. In addition to the inserts in the front and rear apron – reminiscent of an underguard –
and the special side skirt covers, the circular foglamps positioned under the headlights add to the hallmark features of a BMW X. Beyond this, the new BMW X1 boasts attractive touches of sporting elegance. At both front and rear, the surfaces painted in body colour now take up a larger area, while the choice of exterior paintwork colours has been augmented by four new variants.
Front view: even more details in the style of a BMW X model.
When viewed from the front, the powerful stance of the new BMW X1 on the road and its aura of quality are now accentuated with even greater intensity. The path of the car’s lines, which converge on the licence plate mount from either side of the BMW kidney grille, follows the V-shaped contours of the bonnet, forging downwards and outwards in the lower section of the bumper to create the sweeping “X” familiar from the BMW X models in higher vehicle segments. The new tripartite air intake is likewise a feature shared by all
BMW X models.
The car’s striking lines go hand in hand with a detailed execution of the body’s surface styling, signalling a vivacious sporty character and lending the front apron a particularly premium appearance. The foglamps are now level with an extra crease line that forms a discreet scoop along the upper edge of the lights and continues into the side walls. The increased surface area painted in body colour similarly adds to the car’s elegance.
The new-design headlights afford a detailed view of the car’s advanced light technology. In the upper area, a chrome-coated accent strip now cuts across the top of the twin circular headlights, while an LED accent light – included as part of the optional xenon light package, complete with LED light rings for the daytime driving lights – ensures the classic BMW focused look.
Side view: characteristic proportions, new exterior mirrors.
The swage line that rises steadily to the rear of the car, a further character line extending the contours of the side glass graphic as it runs rearwards, and powerfully flared wheel arches allow the BMW X1 to project a very distinctive figure side-on. The pronounced side skirts are a signature feature of the
BMW X models, while the side direction indicators are now integrated into the new-design exterior mirrors.
Rear view: focused emphasis on wide and powerful stance.
The premium feel of the new BMW X1 is also underlined at the rear by the new subdivision of apron, bumper and underguard, with the repositioned reflectors now also bordered by surfaces painted in body colour. As a result, the black plastic elements are slimmer, while the silver-coloured underguard has a more striking surface structure. Furthermore, the contours of the tail lights featuring LEDs now flow harmoniously into the line of the tailgate handle. A stronger emphasis on the horizontal lines renders the rear broader and sportier in appearance.
Interior: precise lines, high-quality materials, sophisticated colour scheme.
The modifications to the design of the new BMW X1 interior create an even more vivid showcase of the sporty driving pleasure, cutting-edge versatility and premium feel this car provides. The side of the centre console angled towards the driver is now shallower and boasts a particularly high-grade surface quality. This sharply highlights the driver-focused principle of the cockpit design. The panel for the sound and climate system controls now has a high-gloss black surface to match the air vent surround. 
The new BMW X1 comes as standard with a storage compartment in the centre of the instrument panel. In vehicles featuring an optional navigation system, this houses the central Control Display for the iDrive operating system. Chrome accents on the side surrounds of the onboard monitor highlight this equipment feature. High-quality electroplated surrounds for the gearshift lever and the centre console cup holder as well as a chrome clip on the headlight switch add the finishing touches to the interior’s exclusive ambience.
Engines: wide choice, sporty power curve, outstanding efficiency.
The engine portfolio of the new BMW X1 comprises three petrol and five diesel engines, offering a wider choice than any competitor and making for hallmark BMW sporting performance. Moreover, their high levels of efficiency coupled with comprehensive BMW EfficientDynamics technology endows all models with a further optimised ratio of performance to fuel consumption that is exemplary in the respective competitive field.
The entry-level unit is the 2.0-litre four-cylinder petrol engine in the
BMW X1 sDrive18i featuring VALVETRONIC variable valve timing and variable camshaft control on both intake and exhaust side (double VANOS). It has output of 110 kW and delivers maximum torque of 200 Newton metres, taking the BMW X1 sDrive18i from standstill to 100 km/h in 9.7 seconds. Average fuel consumption in the EU test cycle is 7.7 litres per 100 kilometres with CO2 emissions of 180 grams per kilometre.
The two 2.0-litre four-cylinder engines on the other petrol models come with BMW TwinPower Turbo technology, a package comprising a twin-scroll turbocharger, High Precision Petrol Direct Injection, VALVETRONIC and double-VANOS. The engine powering the BMW X1 sDrive20i and
BMW X1 xDrive20i provides peak output of 135 kW and maximum torque of 270 Newton metres, enabling acceleration from 0 to 100 km/h in 7.4 (BMW X1 sDrive20i) and 7.8 seconds (BMW X1 xDrive20i) respectively. Average fuel consumption is 6.9 to 7.1 litres (BMW X1 sDrive20i) and 7.5 to 7.7 litres per 100 kilometres (BMW X1 xDrive20i), with CO2 figures of 162 to
165 g/km and 176 to 179 g/km respectively (figures based on the EU test cycle, dependent on the tyre format selected). 
The top-of-the-range engine in the BMW X1 xDrive28i boasts
180 kW and 350 Newton metres, taking 6.1 seconds to sprint from zero to 100 km/h. Fuel consumption in the EU cycle is 7.7 to 7.8 litres per 100 kilometres and CO2 emissions are179 to 182 grams per kilometre (depending on the tyre format selected).
The four-cylinder diesel engines available to the new BMW X1 offer a choice of five output levels and two variants of the BMW TwinPower Turbo technology package. An all-aluminium crankcase, a turbocharger with variable intake geometry, and common-rail direct injection using solenoid injectors are features shared by the 2.0-litre power units for the
BMW X1 sDrive16d, BMW X1 sDrive18d, BMW X1 xDrive18d,
BMW X1 sDrive20d, BMW X1 xDrive20d and BMW X1 sDrive20d EfficientDynamics Edition models. Only the BMW X1 sDrive20d and xDrive20d will be offered in South Africa. The new entry-level diesel model, the BMW X1 sDrive16d, has output of 85 kW and maximum torque of 260 Newton metres. It reaches the 100 km/h mark from standstill in 11.5 seconds and average fuel consumption in the EU test cycle is 4.9 litres per 100 kilometres with CO2 emissions of 128 grams per kilometre. For two further models, the four-cylinder diesel provides output of 105 kW and peak torque of 320 Newton metres. They manage the zero to 100 km/h dash in 9.6 (BMW X1 sDrive18d) and 9.9 seconds (BMW X1 xDrive18d) with average fuel consumption in the EU test cycle of 4.9 and 5.5 litres respectively and CO2 figures of 128 and 144 grams per kilometre.


Thanks to their output of 135 kW and torque rising to 380 Newton metres, the BMW X1 sDrive20d and BMW X1 xDrive20d achieve the standard sprint in 7.8 and 8.1 seconds respectively. The resulting driving pleasure is coupled with fuel and CO2 figures in the EU test cycle of 4.9 litres and 129 grams for the BMW X1 sDrive20d and 5.5 litres per 100 kilometres and 145 grams per kilometre for the BMW X1 xDrive20d. Even more impressive is the relationship between sportiness and frugality in the case of the BMW X1 sDrive20d EfficientDynamics Edition. The world’s most fuel-efficient premium vehicle of its kind summons up 120 kW and maximum torque of likewise 380 Newton metres. The sprint from standstill is accomplished in 8.3 seconds and average fuel consumption in the EU test cycle amounts to 4.5 litres per 100 kilometres with CO2 emissions of 119 grams per kilometre.
The new top-line model among the diesels is the BMW X1 xDrive25d. Delivering 160 kW and peak torque of 450 Newton metres, its engine presents a further boost in tractive power. Ensuring instantaneous power development that continues all the way into the high rev ranges is its
multi-stage charging with variable intake geometry for the smaller of the two turbochargers. Common-rail direct injection uses piezo injectors developing a maximum pressure of 2 000 bar. The BMW X1 xDrive25d sprints from the blocks to 100 km/h in 6.8 seconds. Average fuel consumption in the EU test cycle is 5.9 litres per 100 kilometres and CO2 emissions are 154 grams per kilometre.
All engines are combined as standard with newly developed six-speed manual transmissions. Alternatively, all engine variants – with the exception of the BMW X1 sDrive18i, BMW X1 sDrive16d and BMW X1 sDrive20d EfficientDynamics Edition – can be optionally combined with an eight-speed automatic transmission that is unique in this vehicle segment. For the entry-level petrol model there is the option of a six-speed automatic transmission.
Wide-ranging BMW EfficientDynamics technology, ECO PRO mode marks its debut in the BMW X1.
In line with the enhanced engines and transmissions, the final drive of the new BMW X1 and the power divider of the xDrive all-wheel-drive system likewise boast optimised efficiency. All model variants come equipped with Brake Energy Regeneration. Manual models feature an Optimum Shift Indicator and the Auto Start-Stop function – the latter also in conjunction with the eight-speed automatic transmission. Depending on the model-specific configuration, on-demand operation of ancillary units, a disengageable climate compressor and tyres with reduced rolling resistance are also available.
By means of an optional switch in the centre console control panel below the audio system, ECO PRO mode can now also be activated in the new
BMW X1. This supports a relaxed and economy-optimised driving style through targeted adjustments to the accelerator mapping and the shift characteristics of the automatic transmission. Moreover, the output of electrically operated functions such as the seat heating, climate control system and exterior mirror heating are regulated to ensure highly efficient energy management. A special display informs the driver of the extra range gleaned through these measures.
BMW xDrive all-wheel-drive system: intelligent, fast and precise for enhanced driving pleasure.
Five of the eight engines available to the new BMW X1 can transfer their power to the road with the help of BMW xDrive intelligent all-wheel drive.
The top-of-the-range petrol and diesel engine respectively come with xDrive exclusively. An electronically controlled multi-plate clutch allows the system to transfer power variably to the front and rear wheels, thereby guaranteeing maximum traction, the highest possible safety, outstanding handling and optimal power development regardless of weather or road conditions.
By virtue of being integrated with Dynamic Stability Control (DSC), the xDrive control system is able to analyse the driving situation with great precision.
It can thus counteract any tendency towards oversteer or understeer by distributing power as required before the driver is even aware of the need. What’s more, the collaboration between xDrive and DSC enables the Hill Descent Control function (HDC) for safe passage down an incline at an automatically regulated speed.
State-of-the-art suspension technology for agile and safe handling.
The compelling agility of the new BMW X1 is complemented by superior and precisely controllable driving characteristics. Its high-end suspension technology and advanced stability systems strike an ideal balance between driving dynamics and ride comfort coupled with a high degree of active safety. The all-wheel-drive variants feature a double-joint thrust bar axle at the front, while the BMW X1 sDrive20i, BMW X1 sDrive18i,
BMW X1 sDrive20d, BMW X1 sDrive18d and BMW X1 sDrive16d come with a double-joint tie bar axle. Both front axle variants are paired with a five-arm rear axle.
Also contributing to the precise handling of the new BMW X1 are its steering systems with hydraulic or electromechanical power assistance. On the rear-wheel-drive variants, steering assistance is provided with great efficiency by an electric motor which is only activated if steering support is actually required or requested by the driver. The motor consumes no power during straightline driving or steady-state cornering. Servotronic speed-sensitive power assistance is optionally available on all models.
The powerful braking system, with maintains its capability even under extreme loads, is supported by the Dynamic Stability Control system (DSC) which comes as standard. This system incorporates, inter alia, the Anti-lock Braking System (ABS), Dynamic Traction Control (DTC), Cornering Brake Control (CBC) and Dynamic Brake Control (DBC). Further functions include Brake Assist, Fading Compensation and the Brake Drying function.
The BMW X1 sDrive20i, BMW X1 xDrive20i, BMW X1 xDrive28i and
BMW X1 xDrive25d additionally feature the Brake Standby function and Hill Start Assist.
As an option, the all-wheel-drive model variants can specify the Performance Control system for precisely controlled braking pulses along with torque compensation. This provides a corrective measure against the first signs of understeering on slippery surfaces or in particularly dynamic cornering.
All model variants of the BMW X1 are fitted as standard with 17-inch steel or alloy wheels. The range of optionally available alloys in 17, 18 and – for the first time – 19-inch spec has been further extended.
Premiere in the new BMW X1: the BMW xLine and BMW Sport Line.
So that drivers can endow their new BMW X1 with an individual style based on personal preferences, the BMW Lines have been made available to these models for the first time. The BMW xLine allows the sturdy versatility of the compact BMW X model to be overtly emphasised, comprising as it does underguard elements for the front and rear aprons, side skirt covers, air intake and kidney grille slats in Titanium Silver matt finish, as well as exclusive
18-inch alloys in Y-spoke design. The distinctive charisma of the new
BMW X1 is also brought to bear in the interior, starting with entry strips bearing the lettering “BMW xLine”, a sports leather steering wheel with multifunction buttons, Ambient Lighting with colours that vary from white through to orange, as well as exclusive interior trim strips in Dark Copper
high-gloss and floor mats with colour-matched piping. Another exclusive feature of the BMW xLine are seats in the new Carve variant with hardwearing fabric for the seat surface and the centre section of the seatback and high-grade leather for the side supports. In conjunction with the
BMW xLine, Nevada leather upholstery is another option, with the exclusive colour shades Terra and Oyster also used on the door trim panels and the lower section of the dashboard, while the head restraints feature a distinctive embossed “X”. As a further option, interior trim in Fineline Bay matt fine wood finish is available exclusively in combination with the BMW xLine.
The stand-out agility and dynamics of the new BMW X1 within the competitive environment can also be highlighted through exclusive and meticulously matched design and equipment features. Cue for the
BMW Sport Line, which features a front and rear underguard, side skirt covers, air intakes and kidney grille slats in Black high-gloss, tailpipe finishers in Black Chrome, exclusive 17-inch or – depending on the model – 18-inch light alloys in double-spoke style with bicolour surfaces, and entry strips with
“BMW Sport” lettering. In the interior, sport seats upholstered in anthracite fabric with coral red accents, a sports leather steering wheel and gear selector lever with red stitching, interior trim in Black high-gloss finish, floor mats with red piping and Ambient Lighting that can shift in colour from white to orange all contribute to an ambience that is explicitly geared to intensive driving pleasure. Also optionally available are leather sports seats in a choice of two colours, while interior trim strips in Aluminium with accent line are an optional extra exclusive to the BMW Sport Line.
Both BMW Lines are offered as an alternative to the entry-level version.
An M Sport package is also available as an option for the new BMW X1.
Solid body structure, comprehensive safety equipment.
Like all BMW X models, the new BMW X1 boasts a body with high torsional stiffness which, thanks to intelligent lightweight design, pairs extreme robustness with optimised weight. In the interests of passive safety, the impact forces in the event of an accident are diverted along several load paths, absorbed by precisely defined deformation zones and thus kept away from the stable passenger cell.
As well as front and side airbags for the front seats, standard interior equipment includes side curtain head airbags for both rows of seats,
three-point inertia-reel seat belts on all seats, belt latch limiters and belt latch tensioners at the front and ISOFIX child seat mounts in the rear. All restraint systems are controlled by a central electronic system. Immediately after its market launch, the BMW X1 was awarded the maximum 5-star rating in the Euro NCAP crash test.
Interior allows diverse uses with modern functionality.
The new BMW X1 also showcases its versatility when it comes to potential transportation usage. The rear seatback can be split 40 : 20 : 40, with the three sections folding down individually or jointly according to requirements, and can be adjusted in ten stages. The angle of tilt ranges from 31° –
a particularly comfortable angle for passengers – all the way to a near-vertical cargo position of 1°. This facility alone means the luggage space can vary between 360 and 480 litres, with a capacity of 420 litres when the rear seatback is in its normal position. Folding all three seat elements down fully creates a virtually flat cargo floor with a loading capacity of 1 350 litres.
Two 46-inch golf bags can be stowed widthways or, after folding down the central section of the seatback, lengthwise. The through-loading aperture between the outer rear seats can also be used for two snowboards or four pairs of skis. The passenger compartment offers a wide range of storage spaces and compartments of various sizes, as well as generously sized door pockets. Additional transportation potential is opened up by roof rails (in three colour choices), a storage compartment package, a tow bar with removable ball head, and preparation for a rear carrier rack.
Premium character thanks to comprehensive standard equipment and high-grade options.
The further augmented range of standard equipment on the new BMW X1 guarantees driving enjoyment and comfort at premium car level. The scope includes climate control, electrically adjustable heated exterior mirrors, foglamps, LED tail lights, chrome tailpipe finishers, elasticated straps for the front door pockets, a leather-lined steering wheel, an onboard computer, and a sound system with CD player, AUX-IN connection, five loudspeakers and two-line display showing computer data, telephone numbers and music track titles. The range of optional extras includes, among other features, the navigation system Professional with hard disk and a Harman Kardon Surround Sound System, as well as the options of Comfort Access, Automatic Climate Control, panorama glass roof, automatically dimming exterior and rear-view mirrors, electrically operated seat adjustment, a rain sensor and steering wheel heating.
BMW ConnectedDrive, meanwhile, offers a wide choice of options for optimising the convenience, safety and infotainment functions of the car. Adaptive Headlights with cornering function, available in conjunction with the xenon headlight option, illuminate the road based on the steering angle, speed and yaw rate. The new BMW X1 also offers a rain sensor including automatic driving lights control and High-Beam Assistant. Accurate and safe manoeuvring is facilitated by Park Distance Control and the rear-view camera, which relays its images live to the Control Display of the iDrive operating system. The Cruise Control system with braking function, meanwhile, adjusts not only the engine management and braking but also the gear selection of the optional automatic transmission in order to maintain the driver’s pre-selected speed.


BMW Assist, a globally unique mobility service, comprises among other features a telephone information service and the Automatic/Advanced Emergency Call function with automatic detection of the vehicle location. Other innovative technologies allow unlimited Internet use and the integration of the Apple iPhone and other smartphones as well as music players, including the use of Internet-based services. The Apps option enables iPhone users, among other things, to receive Internet radio stations and to display Facebook and Twitter posts on the onboard monitor. Another new function – Real-Time Traffic Information – provides the driver with exceptionally accurate traffic alerts and recommended diversions. However, this feature will not be available in South Africa. 
The new BMW X1 goes on sale in South Africa from September 2012. 


	
	
	
	
	BMW X1 sDrive18i

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	
	
	5 /5

	Length/width/height1) (unladen)
	mm
	
	
	4477/1798/1545

	Wheelbase
	mm
	
	
	2760

	Track, front/rear
	mm
	
	
	1500/1529

	Turning circle
	m
	
	
	11.3

	Tank capacity
	approx. l
	
	
	63

	Cooling system incl heating
	l
	
	
	7.3 (7.9)

	Engine oil2)
	l
	
	
	4.3

	Weight, unladen, to DIN/EU
	kg
	

	
	1430/1505
(1455/1530)

	Max load to DIN
	kg
	
	
	550

	Max permissible weight
	kg
	
	
	1990 (2010)

	Max axle load, front/rear
	kg
	
	
	915 /1135

	Max trailer load,
braked (12%)/unbraked
	kg
	
	
	1700/750

	Max roof load/towbar download
	kg
	
	
	75/80

	Luggage comp capacity
	l
	
	
	420 – 1350

	Air drag
	cd x A
	
	
	0.32 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	
	
	R/4/4

	Engine technology
	 
	Valvetronic fully variable valve control, double-VANOS

	Effective capacity
	cm³
	
	
	1995

	Bore/stroke
	mm
	
	
	90.0/84.0

	Compression ratio
	:1
	
	
	10.5

	Fuel grade
	
	
	
	min RON 91

	Output
	kW/hp
	
	
	110/150

	at
	rpm
	
	
	6400

	Torque
	Nm
	
	
	200

	at
	rpm
	
	
	3600

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	
	
	70/luggage comp

	Alternator
	A/W
	
	
	180/2520

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Aluminium double-joint tie bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	312 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), 
CBC (Cornering Brake Control), DBC Dynamic Brake Control), 
Fading Compensation, Dry Braking function

	Safety equipment
	  
  
	Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, 
crash sensors, Tyre Defect Indicator

	Steering
	
	EPS (Electric Power Steering), optional: Servotronic

	Steering ratio, overall
	:1
	
	
	16.1

	Tyres, front/rear
	
	
	
	225/50 R17 94H

	Rims, front/rear
	
	
	
	7.5J x 17 steel


[image: ]
Specifications.
BMW X1 sDrive18i.




	


	
	
	
	BMW X1 sDrive18i

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call 

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual (optional: six-speed automatic with Steptronic)

	Gear ratios	I
	
	
	
	4.323 (4.065)

	                                  	II
	:1
	
	
	2.456 (2.371)

	                                  	III
	:1
	
	
	1.659 (1.551)

	                                  	IV
	:1
	
	
	1.230 (1.157)

	                                  	V
	:1
	
	
	1.000 (0.853)

	                                  	VI
	:1
	
	
	0.848 (0.674)

	                                   	R
	:1
	
	
	3.938 (3.200)

	Final drive
	:1
	
	
	3.727 (4.444)

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	
	
	13.0 (13.2)

	Output per litre
	kW/l
	
	
	55.1

	Acceleration	0–100 km/h
	s
	
	
	9.7 (10.4)

		0–1000 m
	s
	
	
	31.0 (31.9)

	in 4th/5th gear         80–120 km/h 
	s
	
	
	9.4/12.2 (–/–)

	Top speed
	km/h
	
	
	202 (200)

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle,
front/rear
	
°
	

	

	
18.0/21.5


	Ramp angle
	°
	
	
	16.8

	Ground clearance unladen
	mm
	
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics
standard features
	
	Valvetronic, double-VANOS, Brake Energy Regeneration, 
on-demand operation of ancillary units, EPS (Electric Power Steering), intelligent lightweight design, final drive with optimised 
warm-up running qualities

	
	
	
	
	

	Fuel consumption EU
	
	
	
	

	Urban
	l/100 km
	
	
	10.4 (10.9)

	Extra-urban
	l/100 km
	
	
	6.2 (6.2)

	Combined
	l/100 km
	
	
	7.7 (7.9)

	CO2
	g/km
	
	
	180 (185)

	Emissions rating
	
	
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	
	
	18/19/24



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight)
Figures in brackets apply to automatic transmission
	
1) Height including roof antenna: 1567 mm
2) Oil change quantity


BMW X1 sDrive20i.
BMW X1 xDrive20i.

	
	
	BMW X1 sDrive20i
	
	BMW X1 xDrive20i

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	5/5
	
	5/5

	Length/width/height1) (unladen)
	mm
	4477/1798/1545
	
	4477/1798/1545

	Wheelbase
	mm
	2760
	
	2760

	Track, front/rear
	mm
	1500/1529
	
	1500/1529

	Turning circle
	m
	11.3
	
	11.8

	Tank capacity
	approx. l
	63
	
	63

	Cooling system incl heating
	l
	8.2 (8.5)
	
	8.2 (8.5)

	Engine oil2)
	l
	5.75
	
	5.75

	Weight, unladen, to DIN/EU
	kg
	1485/1560
(1510/1585)
	
	1575/1650
(1590/1665)

	Max load to DIN
	kg
	550
	
	550

	Max permissible weight
	kg
	2035 (2060)
	
	2125 (2140)

	Max axle load, front/rear
	kg
	940/1170
	
	1005/1175

	Max trailer load,
braked (12%)/unbraked
	kg
	1800/750
	
	2000/750

	Max roof load/towbar download
	kg
	75/80
	
	75/80

	Luggage comp capacity
	l
	420 – 1350
	
	420 – 1350

	Air drag
	cd x A
	0.33 x 2.33
	
	0.34 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	R/4/4
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology with twin-scroll turbocharger, High Precision Direct Injection, Valvetronic fully variable valve control and 
double-VANOS fully variable camshaft control

	Effective capacity
	cm³
	1997
	
	1997

	Bore/stroke
	mm
	90.1/84.0
	
	90.1/84.0

	Compression ratio
	:1
	10.0
	
	10.0

	Fuel grade
	
	min RON 91
	
	min RON 91

	Output
	kW/hp
	135/184
	
	135/184

	at
	rpm
	5000–6250
	
	5000 – 6250

	Torque
	Nm
	270
	
	270

	at
	rpm
	1250–4500
	
	1250 – 4500

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	80/luggage comp
	
	80/luggage comp

	Alternator
	A/W
	170/2380
	
	170/2380

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Aluminium double-joint tie bar axle
	
	Double-joint spring strut thrust bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston frame calliper disc brakes

	Diameter
	mm
	312 x 24/vented
	
	312 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	300 x 20/vented
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), 
CBC (Cornering Brake Control), DBC Dynamic Brake Control), 
Dry Braking function, Fading Compensation, Hill Start Assist, 
BMW X1 xDrive20i: DSC integrated with xDrive all-wheel drive, 
HDC (Hill Descent Control), optional: Performance Control

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, crash sensors, Tyre Defect Indicator

	Steering
	
	EPS (Electric Power Steering), optional: Servotronic
	
	Hydraulic rack-and-pinion power steering, optional: Servotronic

	Steering ratio, overall
	:1
	16.1
	
	18.5

	Tyres, front/rear
	
	225/50 R17 94H
	
	225/50 R17 94H

	Rims, front/rear
	
	7.5J x 17 alloy
	
	7.5J x 17 alloy





	


	
	BMW X1 sDrive20i
	
	BMW X1 xDrive20i

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call 

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual (optional: eight-speed automatic with Steptronic)

	Gear ratios	I
	
	3.683 (4.714)
	
	4.110 (4.714)

	                                  	II
	:1
	2.062 (3.143)
	
	2.315 (3.143)

	                                  	III
	:1
	1.313 (2.106)
	
	1.542 (2.106)

	                                  	IV
	:1
	1.000 (1.667)
	
	1.179 (1.667)

	                                  	V
	:1
	0.809 (1.285)
	
	1.000 (1.285)

	                                  	VI
	:1
	0.677 (1.000)
	
	0.846 (1.000)

	                                  	VII
	:1
	– (0.839)
	
	– (0.839)

	                                  	VIII
	:1
	– (0.667)
	
	– (0.667)

	                                   	R
	:1
	3.348 (3.295)
	
	3.727 (3.295)

	Final drive
	:1
	3.909 (3.154)
	
	3.385 (3.154)

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	11.0 (11.2)
	
	11.7 (11.8)

	Output per litre
	kW/l
	67.6
	
	67.6

	Acceleration	0–100 km/h
	s
	7.4 (7.7)
	
	7.8 (7.9)

		0–1000 m
	s
	28.2 (28.6)
	
	28.9 (29.0)

	in 4th/5th gear         80–120 km/h 
	s
	6.7/8.7 (–/–)
	
	7.3/8.7 (–/–)

	Top speed
	km/h
	220 (220)
	
	215 (215)

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle,
front/rear
	
°
	
18.0/21.5

	

	
18.0/21.5

	Ramp angle
	°
	16.8
	
	16.8

	Ground clearance unladen
	mm
	179
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics standard features
	
	Brake Energy Regeneration, Auto Start-Stop function, ECO PRO mode (optional), Optimum Shift Indicator (manual), on-demand operation of ancillary units, EPS (Electric Power Steering) (BMW X1 sDrive20i), final drive with optimised warm-up running qualities, intelligent lightweight design, disengageable climate compressor, map-controlled oil pump, weight and efficiency-optimised power divider (BMW X1 xDrive20i), 
tyres with reduced rolling resistance

	
	
	
	
	

	Fuel consumption EU 3)
	
	
	
	

	with standard tyres

	Urban
	l/100 km
	8.9 (8.7)
	
	9.5 (9.1)

	Extra-urban
	l/100 km
	5.8 (5.2)
	
	6.3 (6.0)

	Combined
	l/100 km
	6.9 (6.7)
	
	7.5 (7.1)

	CO2
	g/km
	162 (157)
	
	176 (167)

	with 8J x 18 wheels and 225/45 R18 tyres,
with 8J x 18 wheels at the front, 9J x 18 at the rear and 225/45 R18 tyres at the front, 255/40 R18 at the rear,
with 8J x 19 wheels at the front, 9J x 19 at the rear and 225/40 R19 tyres at the front, 255/35 R19 at the rear

	Urban
	l/100 km
	9.0 (8.8)
	
	9.7 (9.2)

	Extra-urban
	l/100 km
	5.9 (5.3)
	
	6.5 (6.2)

	Combined
	l/100 km
	7.1 (6.8)
	
	7.7 (7.3)

	CO2
	g/km
	165 (160)
	
	179 (170)

	Emissions rating
	
	EU5
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	17/19/24
	
	17/19/24



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight)
Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity
3) Fuel consumption and CO2 emissions figures dependent on the selected tyre format


BMW X1 xDrive28i.
	
	
	
	
	BMW X1 xDrive28i

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	
	
	5/5

	Length/width/height1) (unladen)
	mm
	
	
	4477/1798/1545

	Wheelbase
	mm
	
	
	2760

	Track, front/rear
	mm
	
	
	1500/1529

	Turning circle
	m
	
	
	11.8

	Tank capacity
	approx. l
	
	
	63

	Cooling system incl heating
	l
	
	
	8.2 (8.5)

	Engine oil2)
	l
	
	
	5.75

	Weight, unladen, to DIN/EU
	kg
	
	
	1580 (1595)/1655 (1670)

	Max load to DIN
	kg
	
	
	550

	Max permissible weight
	kg
	
	
	2130 (2150)

	Max axle load, front/rear
	kg
	
	
	1015/1175

	Max trailer load,
braked (12%)/unbraked
	kg
	
	
	2000/750

	Max roof load/towbar download
	kg
	
	
	75/80

	Luggage comp capacity
	l
	
	
	420 – 1350

	Air drag
	cd x A
	
	
	0.33 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology with twin-scroll turbocharger, High Precision Direct Injection, Valvetronic fully variable valve control and 
double-VANOS fully variable camshaft control

	Effective capacity
	cm³
	
	
	1997

	Bore/stroke
	mm
	
	
	90.1/84.0

	Compression ratio
	:1
	
	
	10.0

	Fuel grade
	
	
	
	min RON 91

	Output
	kW/hp
	
	
	180/245

	at
	rpm
	
	
	5000 – 6500

	Torque
	Nm
	
	
	350

	at
	rpm
	
	
	1250 – 4800

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	
	
	80/luggage comp

	Alternator
	A/W
	
	
	210/2940

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-joint spring strut thrust bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston frame calliper disc brakes

	Diameter
	mm
	
	
	330 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	330 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), 
CBC (Cornering Brake Control), DBC Dynamic Brake Control), Dry Braking function, Fading Compensation, Hill Start Assist, DSC integrated with xDrive all-wheel drive, HDC (Hill Descent Control), optional: Performance Control

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, 
crash sensors, Tyre Defect Indicator

	Steering
	
	Hydraulic rack-and-pinion power steering, optional: Servotronic

	Steering ratio, overall
	:1
	
	
	18.5

	Tyres, front/rear
	
	
	
	225/50 R17 94H

	Rims, front/rear
	
	
	
	7.5J x 17 alloy





	


	
	
	
	BMW X1 xDrive28i

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, Real-Time Traffic Information, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual (optional: eight-speed automatic with Steptronic)

	Gear ratios	I
	
	
	
	4.110 (4.714)

	                                  	II
	:1
	
	
	2.315 (3.143)

	                                  	III
	:1
	
	
	1.542 (2.106)

	                                  	IV
	:1
	
	
	1.179 (1.667)

	                                  	V
	:1
	
	
	1.000 (1.285)

	                                  	VI
	:1
	
	
	0.846 (1.000)

	                                  	VII
	:1
	
	
	– (0.839)

	                                  	VIII
	:1
	
	
	– (0.667)

	                                   	R
	:1
	
	
	3.727 (3.295)

	Final drive
	:1
	
	
	3.385 (3.154)

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	
	
	8.8 (8.9)

	Output per litre
	kW/l
	
	
	90.1

	Acceleration	0–100 km/h
	s
	
	
	6.1 (6.5)

		0–1000 m
	s
	
	
	26.4 (26.8)

	in 4th/5th gear         80–120 km/h 
	s
	
	
	6.0/7.1 (–/–)

	Top speed
	km/h
	
	
	240 (240)

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle,
front/rear
	
°
	

	

	
18.0/21.5

	Ramp angle
	°
	
	
	16.8

	Ground clearance unladen
	mm
	
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics standard features
	
	Brake Energy Regeneration, Auto Start-Stop function, ECO PRO mode (optional), Optimum Shift Indicator (manual), on-demand operation of ancillary units, final drive with optimised warm-up running qualities, intelligent lightweight design, disengageable climate compressor, map-controlled oil pump, weight and efficiency-optimised power divider, 
tyres with reduced rolling resistance

	
	
	
	
	

	Fuel consumption EU 3)
	
	
	
	

	with standard tyres

	Urban
	l/100 km
	
	
	9.7 (9.1)

	Extra-urban
	l/100 km
	
	
	6.4 (6.1)

	Combined
	l/100 km
	
	
	7.7 (7.2)

	CO2
	g/km
	
	
	179 (168)

	With 8J x 18 wheels and 225/45 R18 tyres,
With 8J x 18 wheels at the front, 9J x 18 at the rear and 225/45 R18 tyres at the front, 255/40 R18 at the rear,
With 8J x 19 wheels at the front, 9J x 19 at the rear and 225/40 R19 tyres at the front, 255/35 R19 at the rear

	Urban
	l/100 km
	
	
	9.9 (9.3)

	Extra-urban
	l/100 km
	
	
	6.6 (6.2)

	Combined
	l/100 km
	
	
	7.8 (7.3)

	CO2
	g/km
	
	
	182 (171)

	Emissions rating
	
	
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	
	
	21/22/24



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight, top speed)
[bookmark: _GoBack]Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity
3) Fuel consumption and CO2 emissions figures dependent on the selected tyre format


BMW X1 sDrive16d.

	
	
	BMW X1 sDrive16d

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	
	
	5/5

	Length/width/height1) (unladen)
	mm
	
	
	4477/1798/1545

	Wheelbase
	mm
	
	
	2760

	Track, front/rear
	mm
	
	
	1500/1529

	Turning circle
	m
	
	
	11.3

	Tank capacity
	approx. l
	
	
	61

	Cooling system incl heating
	l
	
	
	7.2

	Engine oil2)
	l
	
	
	5.2

	Weight, unladen, to DIN/EU
	kg
	
	
	1480/1555 

	Max load to DIN
	kg
	
	
	550

	Max permissible weight
	kg
	
	
	2030

	Max axle load, front/rear
	kg
	
	
	940/1155

	Max trailer load,
braked (12%)/unbraked
	kg
	
	
	1800/750

	Max roof load/towbar download
	kg
	
	
	75/80

	Luggage comp capacity
	l
	
	
	420 – 1350

	Air drag
	cd x A
	
	
	0.33 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology: turbocharger with variable intake geometry, common-rail direct injection, 
max injection pressure: 1600 bar

	Effective capacity
	cm³
	
	
	1995

	Bore/stroke
	mm
	
	
	90.0/84.0

	Compression ratio
	:1
	
	
	16.5

	Fuel grade
	
	
	
	diesel

	Output
	kW/hp
	
	
	85/116

	at
	rpm
	
	
	4000

	Torque
	Nm
	
	
	260

	at
	rpm
	
	
	1750 – 3000

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	
	
	80/luggage comp

	Alternator
	A/W
	
	
	175/2450

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-joint spring strut tie bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	312 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), 
CBC (Cornering Brake Control), DBC Dynamic Brake Control), 
Dry Braking function, Fading Compensation

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, 
crash sensors, Tyre Defect Indicator

	Steering
	
	EPS (Electric Power Steering), optional: Servotronic

	Steering ratio, overall
	:1
	
	
	16.1

	Tyres, front/rear
	
	
	
	225/50 R17 94H

	Rims, front/rear
	
	
	
	7.5J x 17 steel





	


	
	BMW X1 sDrive16d

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, Real-Time Traffic Information, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual

	Gear ratios	I
	:1
	
	
	4.002

	                                  	II
	:1
	
	
	2.109

	                                  	III
	:1
	
	
	1.380

	                                  	IV
	:1
	
	
	1.000

	                                  	V
	:1
	
	
	0.781

	                                  	VI
	:1
	
	
	0.645

	                                   	R
	:1
	
	
	3.647

	Final drive
	:1
	
	
	3.231

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	
	
	17.4

	Output per litre
	kW/l
	
	
	42.6

	Acceleration	0–100 km/h
	s
	
	
	11.5

		0–1000 m
	s
	
	
	33.0

	in 4th/5th gear         80–120 km/h 
	s
	
	
	10.4/14.3

	Top speed
	km/h
	
	
	190

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle,
front/rear
	
°
	

	

	
18.0/22.2

	Ramp angle
	°
	
	
	16.8

	Ground clearance unladen
	mm
	
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics standard features
	
	Brake Energy Regeneration, Optimum Shift Indicator, Auto Start-Stop function, ECO PRO mode (optional), EPS (Electric Power Steering), 
on-demand operation of ancillary units, final drive with optimised 
warm-up running qualities, intelligent lightweight design, 
disengageable climate compressor

	
	
	
	
	

	Fuel consumption EU
	
	
	
	

	Urban
	l/100 km
	
	
	5.7

	Extra-urban
	l/100 km
	
	
	4.4

	Combined
	l/100 km
	
	
	4.9

	CO2
	g/km
	
	
	128

	Emissions rating
	
	
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	
	
	3)



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight)
Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity
3) Data not yet available


BMW X1 sDrive18d.
BMW X1 xDrive18d.
	
	
	BMW X1 sDrive18d
	
	BMW X1 xDrive18d

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	5/5
	
	5/5

	Length/width/height 1) (unladen)
	mm
	4477/1798/1545
	
	4477/1798/1545

	Wheelbase
	mm
	2760
	
	2760

	Track, front/rear
	mm
	1500/1529
	
	1500/1529

	Turning circle
	m
	11.3
	
	11.8

	Tank capacity
	approx. l
	61
	
	61

	Cooling system incl heating
	l
	7.2 (7.5)
	
	7.2 (7.5)

	Engine oil2)
	l
	5.2
	
	5.2

	Weight, unladen, to DIN/EU
	kg
	1480/1555
(1495/1570)
	
	1565/1640
(1575/1650)

	Max load to DIN
	kg
	550
	
	550

	Max permissible weight
	kg
	2055 (2130)
	
	2120 (2140)

	Max axle load, front/rear
	kg
	940/1155
	
	1010/1170

	Max trailer load,
braked (12%)/unbraked
	kg
	1800/750
	
	1800/750

	Max roof load/towbar download
	kg
	75/80
	
	75/80

	Luggage comp capacity
	l
	420 – 1350
	
	420 – 1350

	Air drag
	cd x A
	0.33 x 2.33
	
	0.34 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	R/4/4
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology: turbocharger with variable intake geometry, common-rail direct injection, 
max injection pressure: 1600 bar

	Effective capacity
	cm³
	1995
	
	1995

	Bore/stroke
	mm
	90.0/84.0
	
	90.0/84.0

	Compression ratio
	:1
	16.5
	
	16.5

	Fuel grade
	
	diesel
	
	diesel

	Output
	kW/hp
	105/143
	
	105/143

	at
	rpm
	4000
	
	4000

	Torque
	Nm
	320
	
	320

	at
	rpm
	1750 – 2750
	
	1750 – 2750

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	80/luggage comp
	
	80/luggage comp

	Alternator
	A/W
	175/2450
	
	175/2450

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Aluminium double-joint 
tie bar axle
	
	Double-joint spring strut thrust bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston frame calliper disc brakes

	Diameter
	mm
	312 x 24/vented
	
	312 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	300 x 20/vented
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), CBC (Cornering Brake Control), DBC Dynamic Brake Control), Dry Braking function, Fading Compensation, BMW X1 xDrive18d: DSC integrated with xDrive all-wheel drive, HDC (Hill Descent Control), optional: Performance Control

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, 
crash sensors, Tyre Defect Indicator

	Steering
	
	EPS (Electric Power Steering), optional: Servotronic
	
	Hydraulic rack-and-pinion power steering, optional: Servotronic

	Steering ratio, overall
	:1
	16.1
	
	18.5

	Tyres, front/rear
	
	225/50 R17 94H
	
	225/50 R17 94H

	Rims, front/rear
	
	7.5J x 17 steel
	
	7.5J x 17 steel





	


	
	BMW X1 sDrive18d
	
	BMW X1 xDrive18d

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, Real-Time Traffic Information, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual 
(optional: eight-speed automatic with Steptronic)

	Gear ratios	I
	
	4.002 (4.714)
	
	4.110 (4.714)

	                                  	II
	:1
	2.109 (3.143)
	
	2.248 (3.143)

	                                  	III
	:1
	1.380 (2.106)
	
	1.403 (2.106)

	                                  	IV
	:1
	1.000 (1.667)
	
	1.000 (1.667)

	                                  	V
	:1
	0.781 (1.285)
	
	0.802 (1.285)

	                                  	VI
	:1
	0.645 (1.000)
	
	0.659 (1.000)

	                                  	VII
	:1
	– (0.839)
	
	– (0.839)

	                                  	VIII
	:1
	– (0.667)
	
	– (0.667)

	                                   	R
	:1
	3.647 (3.295)
	
	3.727 (3.295)

	Final drive
	:1
	3.231 (2.929)
	
	3.462 (2.929)

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	14.1 (14.2)
	
	14.9 (15.0)

	Output per litre
	kW/l
	52.6
	
	52.6

	Acceleration	0–100 km/h
	s
	9.6 (9.9)
	
	9.9 (10.1)

		0–1000 m
	s
	30.8 (31.4)
	
	31.5 (31.7)

	in 4th/5th gear         80–120 km/h 
	s
	8.2/10.9 (–/–)
	
	8.7/10.7 (–/–)

	Top speed
	km/h
	202 (202)
	
	195 (195)

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle,
front/rear
	
°
	
18.0/21.5

	

	
18.0/21.5

	Ramp angle
	°
	16.8
	
	16.8

	Ground clearance unladen
	mm
	179
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics
standard features
	
	Brake Energy Regeneration, Auto Start-Stop function, ECO PRO mode (optional), Optimum Shift Indicator (manual), on-demand operation of ancillary units, EPS (Electric Power Steering) (BMW X1 sDrive18d), final drive with optimised warm-up running qualities, intelligent lightweight design, disengageable climate compressor, weight and efficiency-optimised 
power divider (BMW X1 xDrive18d)

	
	
	
	
	

	Fuel consumption EU
	
	
	
	

	Urban
	l/100 km
	5.7 (5.6)
	
	6.5 (6.1)

	Extra-urban
	l/100 km
	4.4 (4.7)
	
	4.8 (5.1)

	Combined
	l/100 km
	4.9 (5.0)
	
	5.5 (5.4)

	CO2
	g/km
	128 (132)
	
	144 (143)

	Emissions rating
	
	EU5
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	19/20/25
	
	19/20/25



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight)
Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity


BMW X1 sDrive20d
EfficientDynamics Edition.

	
	
	BMW X1 sDrive20d EfficientDynamics Edition

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	
	
	5/5

	Length/width/height1) (unladen)
	mm
	
	
	4477/1798/1545

	Wheelbase
	mm
	
	
	2760

	Track, front/rear
	mm
	
	
	1500/1529

	Turning circle
	m
	
	
	11.3

	Tank capacity
	approx. l
	
	
	61

	Cooling system incl heating
	l
	
	
	7.2

	Engine oil2)
	l
	
	
	5.2

	Weight, unladen, to DIN/EU
	kg
	
	
	1490/1565 

	Max load to DIN
	kg
	
	
	550

	Max permissible weight
	kg
	
	
	2045

	Max axle load, front/rear
	kg
	
	
	940/1160

	Max trailer load,
braked (12%)/unbraked
	kg
	
	
	1700/750

	Max roof load/towbar download
	kg
	
	
	75/80

	Luggage comp capacity
	l
	
	
	420 – 1350

	Air drag
	cd x A
	
	
	0.32 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology: turbocharger with variable intake geometry, common-rail direct injection, 
max injection pressure: 1800 bar

	Effective capacity
	cm³
	
	
	1995

	Bore/stroke
	mm
	
	
	90.0/84.0

	Compression ratio
	:1
	
	
	16.5

	Fuel grade
	
	
	
	diesel

	Output
	kW/hp
	
	
	120/163

	at
	rpm
	
	
	4000

	Torque
	Nm
	
	
	380

	at
	rpm
	
	
	1750 – 2750

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	
	
	80/luggage comp

	Alternator
	A/W
	
	
	180/2520

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-joint spring strut tie bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	312 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), 
CBC (Cornering Brake Control), DBC Dynamic Brake Control), 
Dry Braking function, Fading Compensation

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, 
crash sensors, Tyre Defect Indicator

	Steering
	
	EPS (Electric Power Steering), optional: Servotronic

	Steering ratio, overall
	:1
	
	
	16.1

	Tyres, front/rear
	
	
	
	225/50 R17 94W

	Rims, front/rear
	
	
	
	7.5J x 17 alloy





	


	
	BMW X1 sDrive20d EfficientDynamics Edition

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, Real-Time Traffic Information, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual

	Gear ratios	I
	
	
	
	4.110

	                                  	II
	:1
	
	
	2.248

	                                  	III
	:1
	
	
	1.403

	                                  	IV
	:1
	
	
	1.000

	                                  	V
	:1
	
	
	0.802

	                                  	VI
	:1
	
	
	0.659

	                                   	R
	:1
	
	
	3.727

	Final drive
	:1
	
	
	2.929

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	
	
	12.4

	Output per litre
	kW/l
	
	
	60.2

	Acceleration	0–100 km/h
	s
	
	
	8.3

		0–1000 m
	s
	
	
	29.3

	in 4th/5th gear	80–120 km/h 
	s
	
	
	7.1/9.5

	Top speed
	km/h
	
	
	215

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle, front/rear
	
°
	

	

	18.0/22.2

	Ramp angle
	°
	
	
	16,8

	Ground clearance unladen
	mm
	
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics
standard features
	
	Brake Energy Regeneration, Optimum Shift Indicator, Auto Start-Stop function, ECO PRO mode (optional), EPS (Electric Power Steering), 
on-demand operation of ancillary units, final drive with optimised 
warm-up running qualities, intelligent lightweight design, 
disengageable climate compressor, tyres with reduced rolling resistance

	
	
	
	
	

	Fuel consumption EU
	
	
	
	

	Urban
	l/100 km
	
	
	5.2

	Extra-urban
	l/100 km
	
	
	4.1

	Combined
	l/100 km
	
	
	4.5

	CO2
	g/km
	
	
	119

	Emissions rating
	
	
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	
	
	3)



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight)
Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity
3) Data not yet available


BMW X1 sDrive20d.
BMW X1 xDrive20d.

	
	
	BMW X1 sDrive20d
	
	BMW X1 xDrive20d

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	5/5
	
	5/5

	Length/width/height 1) (unladen)
	mm
	4477/1798/1545
	
	4477/1798/1545

	Wheelbase
	mm
	2760
	
	2760

	Track, front/rear
	mm
	1500/1529
	
	1500/1529

	Turning circle
	m
	11.3
	
	11.8

	Tank capacity
	approx. l
	61
	
	61

	Cooling system incl heating
	l
	7.2 (7.5)
	
	7.2 (7.9)

	Engine oil 2)
	l
	5.2
	
	5.2

	Weight, unladen, to DIN/EU
	kg
	1490/1565
(1500/1575)
	
	1575/1650
(1585/1660)

	Max load to DIN
	kg
	550
	
	550

	Max permissible weight
	kg
	2045 (2060)
	
	2130 (2145)

	Max axle load, front/rear
	kg
	940/1160
	
	1010/1165

	Max trailer load,
braked (12%)/unbraked
	kg
	1800/750
	
	2000/750

	Max roof load/towbar download
	kg
	75/80
	
	75/80

	Luggage comp capacity
	l
	420 – 1350
	
	420 – 1350

	Air drag
	cd x A
	0.33 x 2.33
	
	0.34 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	R/4/4
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology: turbocharger with variable intake geometry, common-rail direct injection, 
max injection pressure: 1800 bar

	Effective capacity
	cm³
	1995
	
	1995

	Bore/stroke
	mm
	90.0/84.0
	
	90.0/84.0

	Compression ratio
	:1
	16.5
	
	16.5

	Fuel grade
	
	diesel
	
	diesel

	Output
	kW/hp
	135/184
	
	135/184

	at
	rpm
	4000
	
	4000

	Torque
	Nm
	380
	
	380

	at
	rpm
	1750 – 2750
	
	1750 – 2750

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	80/luggage comp
	
	80/luggage comp

	Alternator
	A/W
	175/2450
	
	175/2450

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Aluminium double-joint 
tie bar axle
	
	Double-joint spring strut thrust bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston frame calliper disc brakes

	Diameter
	mm
	312 x 24/vented
	
	312 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	300 x 20/vented
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), CBC (Cornering Brake Control), DBC (Dynamic Brake Control), Dry Braking function, Fading Compensation, BMW X1 xDrive20d: DSC integrated with xDrive all-wheel drive, HDC (Hill Descent Control), optional: Performance Control

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, 
crash sensors, Tyre Defect Indicator

	Steering
	
	EPS (Electric Power Steering), optional: Servotronic
	
	Hydraulic rack-and-pinion power steering, optional: Servotronic

	Steering ratio, overall
	:1
	16.1
	
	18.5

	Tyres, front/rear
	
	225/50 R17 94H
	
	225/50 R17 94H

	Rims, front/rear
	
	7.5J x 17 steel
	
	7.5J x 17 alloy





	


	
	BMW X1 sDrive20d
	
	BMW X1 xDrive20d

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, Real-Time Traffic Information, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual 
(optional: eight-speed automatic with Steptronic)

	Gear ratios	I
	
	4.110 (4.714)
	
	4.110 (4.714)

		II
	:1
	2.248 (3.143)
	
	2.248 (3.143)

		III
	:1
	1.403 (2.106)
	
	1.403 (2.106)

		IV
	:1
	1.000 (1.667)
	
	1.000 (1.667)

		V
	:1
	0.802(1.285)
	
	0.802 (1.285)

		VI
	:1
	0.659 (1.000)
	
	0.659 (1.000)

		VII
	:1
	– (0.839)
	
	– (0.839)

		VIII
	:1
	– (0.667)
	
	– (0.667)

		R
	:1
	3.727 (3.295)
	
	3.727 (3.295)

	Final drive
	:1
	3.385 (2.929)
	
	3.462 (2.929)

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	11.0 (11.1)
	
	11.7 (11.7)

	Output per litre
	kW/l
	67.7
	
	67.7

	Acceleration	0–100 km/h
	s
	7.8 (7.9)
	
	8.1 (8.1)

		0–1000 m
	s
	28.6 (28.8)
	
	29.1 (29.1)

	in 4th/5th gear	80–120 km/h 
	s
	6.1/7.8 (–/–)
	
	6.5/8.4 (–/–)

	Top speed
	km/h
	220 (218)
	
	215 (213)

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle, front/rear
	
°
	18.0/21.5

	

	18.0/21.5

	Ramp angle
	°
	16.8
	
	16.8

	Ground clearance unladen
	mm
	179
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics
standard features
	
	Brake Energy Regeneration, Auto Start-Stop function, ECO PRO mode (optional), Optimum Shift Indicator (manual), on-demand operation of ancillary units, EPS (Electric Power Steering) (BMW X1 sDrive20d), final drive with optimised warm-up running qualities, intelligent lightweight design, disengageable climate compressor, weight and efficiency-optimised 
power divider (BMW X1 xDrive20d)

	
	
	
	
	

	Fuel consumption EU
	
	
	
	

	Urban
	l/100 km
	5.8 (5.6)
	
	6.6 (6.1)

	Extra-urban
	l/100 km
	4.4 (4.7)
	
	4.9 (5.1)

	Combined
	l/100 km
	4.9 (5.0)
	
	5.5 (5.4)

	CO2
	g/km
	129 (132)
	
	145 (143)

	Emissions rating
	
	EU5
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	20/22/25
	
	20/22/25



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight, top speed)
Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity


BMW X1 xDrive25d.

	
	
	
	
	BMW X1 xDrive25d

	
	
	
	
	

	Body
	
	
	
	

	No of doors/seats
	
	
	
	5/5

	Length/width/height 1) (unladen)
	mm
	
	
	4477/1798/1545

	Wheelbase
	mm
	
	
	2760

	Track, front/rear
	mm
	
	
	1500/1529

	Turning circle
	m
	
	
	11.8

	Tank capacity
	approx. l
	
	
	61

	Cooling system incl heating
	l
	
	
	7.9

	Engine oil2)
	l
	
	
	5.2

	Weight, unladen, to DIN/EU
	kg
	
	
	1585 (1595)/1660 (1670)

	Max load to DIN
	kg
	
	
	550

	Max permissible weight
	kg
	
	
	2150 (2160)

	Max axle load, front/rear
	kg
	
	
	1015/1160

	Max trailer load,
braked (12%)/unbraked
	kg
	
	
	2000/750

	Max roof load/towbar download
	kg
	
	
	75/80

	Luggage comp capacity
	l
	
	
	420 – 1350

	Air drag
	cd x A
	
	
	0.34 x 2.33

	
	
	
	
	

	Engine
	
	
	
	

	Configuration/No of cyls/valves
	
	
	
	R/4/4

	Engine technology
	 
	BMW TwinPower Turbo technology: multi-stage charging with two turobchargers, common-rail direct injection with piezo injectors, 
maximum injection pressure: 2000 bar

	Effective capacity
	cm³
	
	
	1995

	Bore/stroke
	mm
	
	
	90.0/84.0

	Compression ratio
	:1
	
	
	16.5

	Fuel grade
	
	
	
	diesel

	Output
	kW/hp
	
	
	160/218

	at
	rpm
	
	
	4000

	Torque
	Nm
	
	
	450

	at
	rpm
	
	
	1500 – 2500

	
	
	
	
	

	Electrical system
	
	
	
	

	Battery/Installation
	Ah/–
	
	
	80/luggage comp

	Alternator
	A/W
	
	
	175/2450

	
	
	
	
	

	Driving dynamics and safety
	

	Suspension, front
	
	Double-joint spring strut thrust bar axle

	Suspension, rear
	
	Five-arm axle with longitudinal control arm and double wishbone

	Brakes, front
	
	Single-piston frame calliper disc brakes

	Diameter
	mm
	
	
	330 x 24/vented

	Brakes, rear
	
	Single-piston floating calliper disc brakes

	Diameter
	mm
	
	
	300 x 20/vented

	Driving stability systems
	  
  
	Standard: DSC incl ABS and DTC (Dynamic Traction Control), CBC (Cornering Brake Control), DBC Dynamic Brake Control), Dry Braking function, Fading Compensation, Hill Start Assist, DSC integrated with xDrive all-wheel drive, 
HDC (Hill Descent Control), optional: Performance Control Control

	Safety equipment
	  
  
	Standard: Airbags for driver and front passenger, side airbags for driver and front passenger, head airbags front and rear, three-point inertia-reel seatbelts on all seats with belt latch tensioner and belt force limiter in the front, crash sensors, Tyre Defect Indicator

	Steering
	
	Hydraulic rack-and-pinion power steering, optional: Servotronic

	Steering ratio, overall
	:1
	
	
	18.5

	Tyres, front/rear
	
	
	
	225/50 R17 94H

	Rims, front/rear
	
	
	
	7.5J x 17 alloy





	


	
	
	
	BMW X1 xDrive25d

	
	
	
	
	

	BMW ConnectedDrive
	
	
	
	

	Convenience
	
	Optional: BMW Assist incl inter alia Enquiry Service, remote-control functions, BMW TeleServices, integration of mobile devices

	Infotainment
	
	Optional: Internet access, BMW Online incl inter alia Park Info, National Info, Google Local Search, News, Realtime Weather, BMW Routes, Office functions, Bluetooth Audio Streaming, Online Update Music Tracks, Apps

	Safety
	
	Optional: Adaptive Headlights with cornering lights, High-Beam Assistant, 
Park Distance Control, rear-view camera, Cruise Control with braking function, Automatic/Advanced Emergency Call 

	
	
	
	
	

	Transmission
	
	
	
	

	Type of gearbox
	
	Six-speed manual 
(optional: eight-speed automatic with Steptronic)

	Gear ratios	I
	
	
	
	4.110 (4.714)

	                                  	II
	:1
	
	
	2.248 (3.143)

	                                  	III
	:1
	
	
	1.403 (2.106)

	                                  	IV
	:1
	
	
	1.000 (1.667)

	                                  	V
	:1
	
	
	0.802 (1.285)

	                                  	VI
	:1
	
	
	0.659 (1.000)

	                                  	VII
	:1
	
	
	– (0.839)

	                                  	VIII
	:1
	
	
	– (0.667)

	                                   	R
	:1
	
	
	3.727 (3.295)

	Final drive
	:1
	
	
	3.636 (2.929)

	
	
	
	
	

	Performance
	
	
	
	

	Power-to-weight ratio (DIN)
	kg/kW
	
	
	9.9 (10.0)

	Output per litre
	kW/l
	
	
	80.2

	Acceleration	0–100 km/h
	s
	
	
	6.8 (6.8)

		0–1000 m
	s
	
	
	27.5 (27.5)

	in 4th/5th gear         80–120 km/h 
	s
	
	
	5.3/6.6 (–/–)

	Top speed
	km/h
	
	
	230 (228)

	
	
	
	
	

	Offroad specifications
	
	
	
	

	Overhang angle, front/rear
	
°
	

	

	18.0/21.5

	Ramp angle
	°
	
	
	16.8

	Ground clearance unladen
	mm
	
	
	179

	
	
	
	
	

	BMW EfficientDynamics
	
	
	
	

	BMW EfficientDynamics standard features
	
	Brake Energy Regeneration, Auto Start-Stop function, ECO PRO mode (optional), Optimum Shift Indicator (manual), on-demand operation of ancillary units, final drive with optimised warm-up running qualities, intelligent lightweight design, disengageable climate compressor, weight and efficiency-optimised power divider

	
	
	
	
	

	Fuel consumption EU
	
	
	
	

	Urban
	l/100 km
	
	
	7.2 (6.3)

	Extra-urban
	l/100 km
	
	
	5.0 (5.1)

	Combined
	l/100 km
	
	
	5.9 (5.5)

	CO2
	g/km
	
	
	154 (145)

	Emissions rating
	
	
	
	EU5

	
	
	
	
	

	Insurance group
	
	
	
	

	KH/VK/TK
	
	
	
	3)



Specifications apply to ACEA markets; data relevant to homologation applicable in part only to Germany (weight, top speed)
Figures in brackets apply to automatic transmission

1) Height including roof antenna: 1567 mm
2) Oil change quantity
3) Data not yet available


Exterior and interior dimensions.[image: ]
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