

10.Technical specifications

320i; 325i; 330i; 320d

	Body


Anzahl Türen / s
	
	320i
	325i
	330i
	                           320d

	No. of doors/seats

l
	
	4/5
	4/5
	4/5
	4/5

	Length/width/height (unladen) 

)
	mm
	4,520/1,817/1,421
	4,520/1,817/1,421
	4,520/1,817/1,421
	4,520/1,817/1,421

	Wheelbase
	mm
	2,760
	2,760
	2,760
	2,760

	Track, front/rear


	mm
	1,500/1,513
	1,500/1,513
	1,500/1,513
	1,500/1,513

	Turning circle
	m
	11.0
	11,0
	11.0
	11.0

	Fuel tank capacity
	approx. ltr
	60
	60
	60
	60

	Cooling system incl. heating

l
	ltr
	7.5 (8.1)
	8.2 (8.5)
	8.2 (8.5)
	7.5 (7.9)

	Engine oil


	ltr
	4.25
	6.5
	6.5
	5.5

	Transmission fluid
	ltr
	Permanent filling
	Permanent filling
	Permanent filling
	Permanent filling

	Final drive fluid
	ltr
	Permanent filling
	Permanent filling
	Permanent filling
	Permanent filling

	Weight, unladen (EU1)
	kg
	1,395 (1,425)
	1,490 (1,520)
	1,525 (1,540)
	1,490 (1,505)

	Max load (DIN)
	kg
	520
	520
	520
	520

	Max. permissible weight (DIN)
	kg
	1,840 (1,870)
	1,935 (1,965)
	1,970 (1,985)
	1,935 (1,950)

	Permissible axle load front/rear
	kg
	870/1,035
	925 (1,075)
	935/1,085
	925/1,060

	Max. trailer load2
	
	
	
	
	

	braked (12%)/unbraked


	kg
	1,400 (1,500)/695
	1,600 (1,700)/745
	1,700 (1,800)/750
	1,600/745

	Max. roof load/trailer nose weight
	kg
	75/75
	75/75
	75/75
	75/75

	Luggage comp. capacity VDAKofferrauminhalt nach VDA
	ltr
	460
	460
	460
	460

	Drag coefficient
	cX x A
	0.28 x 2.11
	0.30 x 2.11
	0.30 x 2.11
	0.29 x 2.11

	Engine
	
	
	
	
	

	Layout/No. of cylinders/Valves Zylinder/Ventile


	
	Inline/4/4
	Inline/6/4
	Inline/6/4
	Inline/4/4

	Engine management
	
	MEV9
	MSV70
	MSV70
	DDE6

	Displacement
	cc
	1,995
	2,497
	2,996
	1,995

	Bore/Stroke
	mm
	84.0/90.0
	78.8/82.0
	85.0/88.0
	84.0/90.0

	Compression ratio


	:1
	10.5 
	11.0
	10.7
	17.0

	Fuel grade3
	RON
	91–98
	91–98
	91–98
	Diesel

	Max. output
	bhp
	150
	218
	258
	163

	At engine speed
	rpm
	6,200
	6,500
	6,600
	4,000

	Torque
	Nm
	200
	250
	300
	340

	At engine speed
	rpm
	3,600
	2,750–4,250
	2,500–4,000
	2,000

	Electrics
	
	
	
	
	

	Battery/Location
	Ah/–
	46/boot
	70/boot
	70/boot
	80/boot

	Alternator
	A/W
	110/1,540
	155/2,170
	155/2,170
	150/2,100

	Chassis
	
	
	
	
	

	Front suspension
	
	Double-joint spring-strut suspension with displaced camber; 
small positive steering scrub radius; traverse force compensation; anti-dive

	Rear suspension
	
	Independent 5-arm axle, steel-lightweight construction

	Brakes, front
	
	Single-piston floating-caliper disc brakes

	Diameter
	mm
	292 x 22, vented
	300 x 24, vented
	330 x 24, vented
	300 x 24, vented

	Brakes, rear
	
	Single-piston floating-caliper disc brakes

	Diameter
	mm
	296 x 10, vented
	    300 x 20, vented
	336 x 22, vented
	     300 x 20, vented

	Driving Stability Systems
	
	ABS, Traction Control (ASC+T), wheel-selective Electronic Braking Distribution (EBD,CBC), Dynamic Stability Control (DSC), Electronic Differential Lock (ADB), 
Dynamic Brake Control (DBC)

	Steering
	
	Rack-and- pinion, power-assisted; 3.0 turns lock to lock

	Overall ratio
	:1
	16,0
	16,0
	16,0
	16,0

	Type of transmission
	
	6-gear manual; 6-gear sequential manual transmission (for 325i and 330i) as an option; 
6-gear Steptronic automatic transmission as an option

	Transmission ratio
I

  
	:1
	4.32 (4.17)
	4.32 (4.17)
	4.35 (4.17)
	5.14 (4.17)

	                                  
II
	:1
	2.46 (2.34)
	2.46 (2.34)
	2.50 (2.34)
	2.83 (2.34)

	                                  
III
	:1
	1.66 (1.52)
	1.66 (1.52)
	1.67 (1.52)
	1.80 (1.52)

	                                  
IV
	:1
	1.23 (1.14)
	1.23 (1.14)
	1.23 (1.14)
	1.26 (1.14)

	                                  
V
	:1
	1.00 (0.87)
	1.00 (0.87)
	1.00 (0.87)
	1.00 (0.87)

	                                  
VI
	:1
	0.85 (0.69)
	0.85 (0.69)
	0.85 (0.69)
	0.83 (0.69)

	                                  
R
	:1
	3.94 (3.40)
	3.94 (3.40)
	3.93 (3.40)
	4.64 (3.40)

	Final drive ratio
	:1
	3.38 (3.91)
	3.23 (3.73)
	3.15 (3.64)
	2.56 (3.15)

	Tyres 
	
	205/55 R 16 91 V
	205/55 R 16 91 W
	225/45 R 17 91W
	205/55 R 16 91 V

	Wheels 
	
	7 J x 16 steel LLichtbauBS-Rad 
	7 J x 16 steel LLichtbauBS-Rad 
	8 J x 17 alloy
	7 J x 16 steel

	Performance
	
	
	
	
	

	Acceleration      0–62mph
	sec
	9.0 (9.7)
	7.0 (7.7)
	6,3 (6,6)
	8.3 (8.6)

	                           0–1,000 m
	sec
	29.9 (30.7)
	27.4 (28.1)
	26.2 (26.2)
	29.3 (29.5)

	50–75 mph in 4th gear
	sec
	8.9 (–)
	7.5 (–)
	6.5 (–)
	6.5 (–)

	Top speed4
	mph
	137 (134)
	152 (150)
	155 (155)
	140 (137)

	Fuel consumption (EU cycle)
	
	
	
	
	

	In town
	mpg
	26.4 (25.7)
	23.3 (21.0)
	22.2 (21.0)
	36.2 (31.0)

	Out of town
	mpg
	50.4 (45.6)
	45.6 (42.2)
	44.1 (41.5)
	62.8 (53.3)

	Overall
	mpg
	38.2 (35.8) 
	33.6 (31.4)
	32.5 (31.4)
	49.6 (43.2)

	CO2 
	g/km
	178 (190)
	203 (218)
	210 (216)
	153 (179)

	Miscellaneous
	
	
	
	
	

	Emission classification
	
	EU4 
	EU4 
	EU4 
	EU4 


The values given in parenthesis apply to the automatic transmission.

1Weight of the car in road trim (DIN) plus 75 kg for driver and luggage.


2Deviations are possible under certain conditions.


3Information about performance and fuel consumption relate to RON 98.
4Electronically.




































