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2003 BMW 760Li Specifications

Bold within table indicates new specification relative to 2003 745Li.

General

Curb weight, lb.
4872

GVWR, lb.
5930
Weight distribution, front/rear, %
51.6/48.4
Wheelbase, in.
123.2

Track, front/rear, in.


Length, in.
203.5

Width, in.
74.9


Height, in.
58.7

Accommodations

Seating capacity, persons
5


Shoulder room, front/rear, in.
59.3/58.9

Leg room, front/rear
41.9/43.4

Headroom, front/rear
39.2/38.5

EPA interior volume, cu ft.
111.0

EPA cargo volume, cu ft.
18.0 

Body
Type
4-door sedan

Aerodynamic drag coefficient (CD)
0.29

EPA size classification
Large
Engine & electrical

Engine type
DOHC (4-cam) 48-valve V-12,



direct fuel injection, Valvetronic



variable valve lift & Double VANOS 



steplessly variable intake- &



exhaust-valve timing

Cylinder block & heads
Aluminum

Bore x stroke, mm/in.
89.0 x 80.0 / 3.50 x 3.15
Displacement, cc/cu in.
5972/364
Compression ratio
11.3:1
Power @ rpm, hp
438 @ 6000

Torque @ rpm, lb-ft.
444 @ 3950
Engine-management system
Motronic MED9
Fuel requirement
Premium unleaded
Fuel capacity, U.S. gal.
23.3
Battery capacity, amp-hr.
110
Alternator output, amp./W
180/2520
Drivetrain
Drive system
Front engine/rear drive
Automatic transmission
ZF 6HP26, 6-speed
Ratios:
1st
4.17:1


2nd
2.34:1


3rd
1.52:1



4th
1.14:1



5th
0.87:1



6th
0.69:1



Reverse
3.40:1

Final drive ratio
3.15:1
Chassis

Body/frame construction
Unitized all-steel structure with



aluminum hood & front fenders
Front suspension
Strut-type in aluminum; double-pivot



lower arms, coil springs, twin-tube



gas-pressure shock absorbers &



Electronic Damping Control,



Active Roll Stabilization;



aluminum subframe

Rear suspension
4-link integral suspension in



aluminum, self-leveling air springs,



twin-tube gas-pressure shock



absorbers & Electronic Damping



Control, Active Roll Stabilization;



aluminum subframe

Steering type
Rack & pinion, vehicle-speed-sensitive,



power assist & variable ratio

Turns lock-to-lock
3.07

Turning circle, ft.
41.3

4-wheel ventilated disc brakes:


Front, diameter x thickness, mm.
348 x 30


                                                                          inch
13.7 x 1.18


Rear, diameter x thickness, mm/in.
345 x 24 


                                            Inch
13.6 x 0.94

Assist
Vacuum
Wheels: 



standard
Forged alloy, 19 x 9.0 front /




19 x 10.0 rear 



optional
Forged alloy, 18 x 8.0


optional
Cast alloy, 18 x 8.0 for run-flat tires
Tires:



standard
245/45R-19 front /




275/40R-19 rear performance 



optional
245/50R-18 V-rated all-season


optional
245/50R-18 V-rated all-season run-flat
Chassis (cont.)

Stability-enhancement system
Dynamic Stability Control (DSC),




encompassing Dynamic Traction




Control, antilock braking (ABS),




electronic brake proportioning,




Dynamic Brake Control & cornering/




avoidance stability enhancement

Performance data

Acceleration, 0-60 mph, sec.
5.4 

Top speed, mph
149 (electronically limited)

Fuel economy, EPA est. MPG,


City

15 


Highway
23


Combined
18
� – Optional rear climate control & coolbox reduce cargo volume.


� – VANOS = VAriable NOckenwellen Steuerung = variable camshaft control, or variable valve timing.


� – BMW AG test results. Actual acceleration results may vary depending on specification of vehicle; road and environmental conditions; testing procedures and driving style. These results should be used for comparison only, and verification should not be attempted on public roads. BMW urges you to obey all posted speed limits and to please wear your safety belt at all times.
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