Media Information
25 June 2014

**Company**

Bayerische

Motoren Werke

Aktiengesellschaft

**Postal Address**

BMW AG

80788 München

**Telephone**

089-382-28720

**Internet**

www.bmwgroup.com

BMW Group engines secure another double win in the Engine of the Year Award 2014.

Run of success continues with awards in two displacement classes: the 3.0-litre straight-six with BMW TwinPower Turbo technology wins its fourth title and the MINI 1.6-litre four-cylinder turbo unit its eighth in the world's leading engine competition.

Munich / Stuttgart. Two class wins in this year’s competition have boosted the BMW Group’s cache of titles acquired in the prestigious International Engine of the Year Award. The two latest accolades go to two power units that manage to combine sporty performance with exemplary efficiency in unique fashion. The 3.0-litre in-line six-cylinder petrol engine with BMW TwinPower Turbo technology – as featured in numerous current BMW models – ranks among the prize-winners for the fourth time. Meanwhile, the 1.6-litre four-cylinder turbo engine that drives the MINI Cooper S Countryman and the MINI Cooper S Paceman, among other models, has secured its eighth consecutive class win.

This brace of titles for the BMW Group at the International Engine of the Year Award 2014 once again corroborates the development work carried out under the umbrella of Efficient Dynamics, which has for years now led to a steady enhancement in driving pleasure coupled with reduced fuel consumption and emissions. The International Engine of the Year Award was introduced in 1999, since when 63 class and overall wins have been earned by engines developed for the BMW and MINI brands. Deciding on the best engines among a wide range of categories was a panel of expert judges who this year comprised 82 automotive journalists from 34 countries. Their chosen prize-winners will be presented with their awards on Wednesday, 25 June 2014 during the Engine Expo trade fair in Stuttgart.

In the six-in-line petrol engine that has once again won the Engine of the Year Award in 2014, BMW TwinPower Turbo technology plays a pivotal role in securing its hallmark brand attributes: instantaneous response to the slightest touch of the pedal, an exhilarating high-revving temperament, supreme refinement and outstanding efficiency. The technology package behind the lightweight unit comprises a Twin Scroll turbocharger, High Precision Petrol Direct Injection, VALVETRONIC variable valve timing and double-VANOS variable camshaft control. With this armoury, the 3.0-litre engine delivers peak output of 225 kW/306 hp and 235 kW/320 hp in the respective BMW 6 Series and BMW 7 Series models.

This year the 1.4 to 1.8-litre displacement class of the International Engine of the Year Award was once again dominated by the 1.6-litre turbocharged engine developed for BMW and MINI models. This unit features a Twin Scroll turbocharger and petrol direct injection combined with variable valve control based on the VALVETRONIC principle patented by the BMW Group. In its latest evolution – available from summer 2014 in the new MINI Cooper S Countryman (fuel consumption combined: 6.0 l/100 km [47.1 mpg imp]; CO2 emissions combined: 139 g/km) and the new MINI Cooper S Paceman (fuel consumption combined: 6.0 l/100 km [47.1 mpg imp]; CO2 emissions combined: 139 g/km) – the four-cylinder powerplant boasts output raised to 140 kW/190 hp. The responsive, high-revving nature and excellent efficiency of this engine once again set benchmarks that have ensured its eighth class win in succession.

Further information on official fuel consumption figures, specific CO2 emission values and the electric power consumption of new passenger cars is included in the following guideline: “Leitfaden über Kraftstoffverbrauch, die CO2-Emissionen und den Stromverbrauch neuer Personenkraftwagen” (Guideline for fuel consumption, CO2 emissions and electric power consumption of new passenger cars), which can be obtained from all dealerships, from the Deutsche Automobil Treuhand GmbH (DAT), Hellmuth-Hirth-Str. 1, 73760 Ostfildern-Scharnhausen and at http://www.dat.de/en/offers/publications/guideline-for-fuel-consumption.html. LeitfadenCO2 (GuidelineCO2) (PDF ‒ 2.7 MB)

**The BMW Group**

With its three brands BMW, MINI and Rolls-Royce, the BMW Group is the world’s leading premium manufacturer of automobiles and motorcycles and also provides premium financial and mobility services. As a global company, the BMW Group operates 28 production and assembly facilities in 13 countries and has a global sales network in more than 140 countries.

In 2013, the BMW Group sold approximately 1.963 million cars and 115,215 motorcycles worldwide. The profit before tax for the financial year 2013 was € 7.91 billion on revenues amounting to approximately € 76.06 billion. As of 31 December 2013, the BMW Group had a workforce of 110,351 employees.

The success of the BMW Group has always been based on long-term thinking and responsible action. The company has therefore established ecological and social sustainability throughout the value chain, comprehensive product responsibility and a clear commitment to conserving resources as an integral part of its strategy.

[www.bmwgroup.com](http://www.bmwgroup.com)

Facebook: <http://www.facebook.com/BMWGroup>

Twitter: <http://twitter.com/BMWGroup>

YouTube: <http://www.youtube.com/BMWGroupview>

Google+: <http://googleplus.bmwgroup.com>

For questions please contact:

Manfred Poschenrieder, Spokesperson Efficient Dynamics

Phone: +49 89-382-28720, Fax: +49 89-382-28567

Cypselus von Frankenberg, Head of Technology Communication

Cypselus.von-Frankenberg@bmw.de

Telefon: +49 89-382-30641, Fax: +49 89-382-28567

Media Website: www.press.bmwgroup.com

E-mail: presse@bmw.de